{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["бетон ","железобетон 10.05.12"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"бетон ","index":0,"n_rows":74,"n_cols":6,"rows_kept":74,"cut":false,"hidden":false,"merged":[[14,0,14,2],[11,0,11,4],[12,0,12,4],[13,0,13,4]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,null,"                                                                                     Утверждаю"]
[null,null,"                                                                                     Генеральный директор"]
[null,null,"                                                                                     ООО \"Смоленский завод ЖБИ-2\""]
[null,null,"                                                                                      ______________ В.Н. Бондарь"]
[]
[null,null,null,"10 мая 2012г.",null,"27 апреля 2010г."]
["ПРАЙС-ЛИСТ"]
["ООО \"Смоленский завод ЖБИ-2\""]
["на смеси бетонные и растворы"]
[]
["8(4812)31-06-59 Планово-экономический отдел"]
["8(4812)31-06-86 Транспортный цех"]
["Email:gbi2smol@yandex.ru"]
["www.gbi-n2.ru"]
[]
["Номенклатура","Класс","Марка","ЦЕНА","ЦЕНА"]
[null,null,null,"м3","м3"]
[null,null,null,"без НДС","с НДС"]
["Смесь бетонная","В7,5","М-100",2266.949152542373,2675]
["Смесь бетонная","В10;В12,5","М-150",2372.8813559322034,2800]
["Смесь бетонная","В10;В12,5","М-150 F75",2741.5254237288136,3235]
["Смесь бетонная","В10;В12,5","М-150 F100",2974.576271186441,3510]
["Смесь бетонная","В15","М-200 ",2491.5254237288136,2940]
["Смесь бетонная","В15","М-200 П-3",2550.8474576271187,3010]
["Смесь бетонная","В15","М-200 П-4",2677.9661016949153,3160]
["Смесь бетонная","В15","М-200 F50,F75,F75W2",2919.491525423729,3445]
["Смесь бетонная","В15","М-200 F100W6, М-200 F200",3631.3559322033902,4285]
["Смесь бетонная","В15","М-200 F150W4,М-200 F100,М-200 W4,М-200 F75W4",3135.5932203389834,3700]
["Смесь бетонная","В20","М-250",2724.576271186441,3215]
["Смесь бетонная","В20","М-250 F200W6, M-250 F200",3631.3559322033902,4285]
["Смесь бетонная","В20","М-250 F75W4, M-250 F100",3220.3389830508477,3800]
["Смесь бетонная","В22,5","М-300 на гравии",2830.5084745762715,3340]
["Смесь бетонная","В22,5","М-300 на щебне",3220.3389830508477,3800]
["Смесь бетонная","B22,5","M-300 П-3",2741.5254237288136,3235]
["Смесь бетонная","B22,5","M-300 П-4",2898.305084745763,3420]
["Смесь бетонная","B22,5","М-300 F50,F75W2,M-300 F100",3220.3389830508477,3800]
["Смесь бетонная","B22,5","M-300 F200, F100W6, F200W6, W6",3631.3559322033902,4285]
["Смесь бетонная","В25;В26,5","М-350",3411.0169491525426,4025]
["Смесь бетонная","B25;В26,5","М 350 П4, F75П4, F75, F100, F150w4",3631.3559322033902,4285]
["Смесь бетонная","B25;В26,5","M350 F200",3631.3559322033902,4285]
["Смесь бетонная","В30","М-400,М-400 F-200, W-6",3745.762711864407,4420]
["Смесь бетонная","B30","M400W6F200, F100W6, F150, F150w4",3745.762711864407,4420]
["Смесь бетонная","В35","М-450 f-200; М-450",3813.5593220338983,4500]
["Смесь бетонная","B35","M450F200W8 мост",4110.169491525424,4850]
["Смесь бетонная","B35","M450F300W8 ",4110.169491525424,4850]
["Смесь бетонная","В40","М-500 f-200; М-500",4004.2372881355936,4725]
["Раствор",null,"М-75",1936.4406779661017,2285]
["Раствор",null,"М-100",2055.084745762712,2425]
["Раствор",null,"М-150",2338.983050847458,2760]
["Раствор",null,"М-200",2614.406779661017,3085]
["Раствор известковый",null,null,2580.5084745762715,3045]
["Раств. Слож. ",null,"М-50",1936.4406779661017,2285]
["Раств. Слож.",null,"М-75",2118.64406779661,2500]
["Раств. Слож. ",null,"М-100",2156.7796610169494,2545]
["Раств. Слож.",null,"М-150",2372.8813559322034,2800]
["Раств. ",null,"М-150 М.П.",0]
["Раств. ",null,"М-75 слож. М.П.",0]
["Раств. ",null,"М-200 М.П.",0]
["Раств. Слож.",null,"М-150 М.П.",0]
["Раствор",null,"М-100 М.П.",0]
["Раствор",null,"М-75 М. П.",0]
["Цементно-песчаная смесь",null," М-400",0]
[null,null,null,0]
[]
["Осуществляем доставку бетонной смеси и раствора"]
["Автомиксер (7,4м3)-1700,00руб./час"]
["Автомиксер (5,6м3)-1500,00руб./час"]
["Автомиксер (3,6м3)-1200,00руб./час"]
["Самосвал ЗИЛ (2,25м3) - 850,00руб./час "]

{"sheet":"железобетон 10.05.12","index":1,"n_rows":478,"n_cols":7,"rows_kept":478,"cut":false,"hidden":false,"merged":[[460,0,460,6],[462,0,462,6],[399,0,399,6],[403,0,403,6],[454,0,454,6],[65,0,65,6],[397,0,397,6],[320,0,320,6],[327,0,327,6],[330,0,330,6],[302,0,302,6],[335,0,335,6],[369,0,369,6],[371,0,371,6],[153,0,153,6],[40,0,40,6],[6,0,6,6],[7,0,7,6],[20,0,20,6],[14,0,14,6],[15,0,15,6],[22,0,22,6],[29,0,29,6],[35,0,35,6],[480,0,480,6],[43,0,43,6],[50,0,50,6],[53,0,53,6],[58,0,58,6],[157,0,157,6],[165,0,165,6],[60,0,60,6],[138,0,138,6],[144,0,144,6]],"flags":["formulas_cached_only"]}
[{"$nulls":5},"    Утверждаю"]
[{"$nulls":5},"Генеральный директор"]
[{"$nulls":5},"ООО \"Смоленский завод ЖБИ-2\""]
[{"$nulls":5},"________________ В.Н. Бондарь"]
[]
[{"$nulls":6},"10 мая 2012 г."]
["ПРАЙС ЛИСТ "]
["ООО \"Смоленский завод ЖБИ-2\""]
[]
["8(4812)31-06-59 Планово-экономический отдел"]
["8(4812)31-07-15 Производственно-технический отдел"]
["Email:gbi2smol@yandex.ru"]
["Email:gbi2info@yandex.ru"]
["www.gbi-n2.ru"]
[]
["Осуществляем поставку щебня,гравия,песка"]
[]
["Марка","ЦЕНА","ЦЕНА","ЦЕНА","объем","Вес","Габариты"]
[null,"шт.","шт.","шт.","1шт ","1 шт. ","Дл. Шир. Высота"]
[null,"без НДС","с НДС","с НДС","м3","тн.","мм."]
["Балки односкатные"]
["2БОЭ12-4АIIIвт",42326.27118644068,35650,49945,2,5,"11960*890*280"]
["Дорожные плиты"]
["2П30.15-30",5364.406779661017,4750,6330,0.765,1.98,"3000*1500*170"]
["2П30.18-30",5961.864406779661,5250,7035,0.88,2.2,"3000*1750*170"]
["1П30.18-30",7983.050847457627,null,9420,0.88,2.2,"3000*1750*170"]
["ПД20.15-17",6601.6949152542375,null,7790,0.61,1.53,"1990*1490*210"]
["ПДГ-1,5-6с",10199.152542372882,9000,12035,1.26,3.15,"1500*6000*140"]
["ПАГ-14V",17016.949152542373,15200,20080,1.68,4.2,"6000*2000*140"]
["Кольца смотровых колодцев"]
["КЦ7-10",1309.322033898305,1100,1545,0.17,0.43,"840/700*70*990"]
["КЦ10-6",1131.3559322033898,950,1335,0.16,0.4,"1160/1000*80*590"]
["КЦ10-9",1724.5762711864409,1450,2035,0.24,0.6,"1160/1000*80*890"]
["КЦ15-6",1779.6610169491526,1500,2100,0.265,0.66,"1680/1500*90*590"]
["КЦ15-9",2614.406779661017,2200,3085,0.4,1,"1680/1500*90*890"]
["Крышки колодцев"]
["КЦП1-10-1",1432.2033898305085,1200,1690,0.1,0.25,"1180*700*180"]
["КЦП1-10-2",1618.6440677966102,null,1910,0.1,0.25,"1180*700*180"]
["КЦП1-15-1",3338.983050847458,null,3940,0.27,0.68,"1680*700*150"]
["КЦП1-15-2",3703.389830508475,2800,4370,0.27,0.68,"1680*700*150"]
["Днища колодцев"]
["КЦД-10",1669.491525423729,1400,1970,0.18,0.45,"1500*100"]
["КЦД-15",3338.983050847458,2800,3940,0.38,0.95,"2000*120"]
["Лестничные марши"]
["1ЛМ27.11.14-4",5495.762711864407,4610,6485,0.531,1.33,"2720*1050"]
["1ЛМ27.12.14-4",6228.813559322034,5230,7350,0.607,1.52,"2720*1200"]
["1ЛМ30.11.15-4",6440.677966101695,5400,7600,0.58,1.45,"3000*1050"]
["1ЛМ30.12.15-4",7360.169491525424,6190,8685,0.68,1.7,"3000*1200"]
["ЛМП57.11.15-5",16144.06779661017,13570,19050,0.92,2.3,"5650*1150"]
["ЛМ58-14-17",18525.42372881356,15570,21860,0.915,2.29,"5770*1150"]
["Лестничные площадки"]
["2ЛП22.18-4к",4381.35593220339,3680,5170,0.547,1.37,"2200*1900"]
["2ЛП25.18-4к",5250,4420,6195,0.623,1.56,"2500*1900"]
["Лотки"]
["Л4-8",6029.661016949153,5070,7115,0.72,1.8,"5970*780*530"]
["Л6-8",8542.372881355932,7180,10080,0.9,2.25,"5970*1160/1000*530"]
["Л7-8",9716.101694915254,8170,11465,1.06,2.65,"5970*1160/980*680"]
["Л11-8",17262.71186440678,14510,20370,1.44,3.6,"5970*1480/1280*700"]
["Опорные подушки"]
["ОП5-4т",453.3898305084746,350,535,0.03,0.08,"510*380*140"]
["Стойки электропередач"]
["СВ 95-2",4059.322033898305,3400,4790,0.3,0.75,"9500*165/150*165/240"]
["СВ 95-3с",4737.28813559322,3970,5590,0.3,0.75,"9500*165/150*165/240"]
["СВ110-3,5",5677.966101694916,4750,6700,0.45,1.13,"11000*185/175*165/280"]
["СВ110-5*",8338.983050847459,7000,9840,0.45,1.13,"11000*185/175*165/280"]
["Перемычки"]
["1ПБ10-1п",186.4406779661017,140,220,0.008,0.02,"1030*120*65"]
["1ПБ13-1п",211.86440677966104,170,250,0.01,0.03,"1290*120*65"]
["1ПП-12-3п",338.98305084745766,260,400,0.029,0.07,"1160*380*65"]
["2ПБ10-1п",237.28813559322035,190,280,0.017,0.04,"1030*120*140"]
["2ПБ13-1п",322.0338983050848,250,380,0.022,0.06,"1290*120*140"]
["2ПБ16-2п",360.3813559322034,285,425.25,0.026,0.07,"1550*120*140"]
["2ПБ17-2п",368.6440677966102,294.5,435,0.028,0.07,"1680*120*140"]
["2ПБ19-3п",389.8305084745763,315,460,0.033,0.08,"1940*120*140"]
["2ПБ22-3п",423.7288135593221,340,500,0.037,0.09,"2200*120*140"]
["2ПБ25-3п",516.9491525423729,410,610,0.041,0.1,"2460*120*140"]
["2ПБ26-4п",546.6101694915254,440,645,0.044,0.11,"2590*120*140"]
["2ПБ29.4п",644.0677966101696,510,760,0.048,0.12,"2850*120*140"]
["2ПБ30-4п",652.542372881356,520,770,0.05,0.13,"2980*120*140"]
["2ПГ39-31",4271.186440677966,3420,5040,0.317,0.79,"3890*250*440"]
["2ПГ44-31п",7144.06779661017,5730,8430,0.359,0.9,"4410*250*440"]
["2ПГ48-31п",7771.186440677967,6240,9170,0.391,0.98,"4800*250*440"]
["2ПП14-4п",652.542372881356,530,770,0.076,0.19,"1420*380*140"]
["2ПП21-6п",1016.949152542373,810,1200,0.11,0.28,"2070*380*140"]
["2ПП23-8п",1245.7627118644068,1000,1470,0.124,0.31,"2330*380*140"]
["3ПБ-13-37п",466.10169491525426,370,550,0.034,0.09,"1290*120*220"]
["3ПБ16-37п",593.2203389830509,470.25,700,0.041,0.1,"1550*120*220"]
["3ПБ18-37-1;2",1122.8813559322034,900,1325,0.048,0.12,"1810*120*220"]
["3ПБ18-37п",652.542372881356,530,770,0.048,0.12,"1810*120*220"]
["3ПБ18-8п",538.3474576271187,430,635.25,0.048,0.12,"1810*120*220"]
["3ПБ21-8п",601.6949152542373,480,710,0.055,0.14,"2070*120*220"]
["3ПБ25-8п",750,610,885,0.066,0.17,"2460*120*220"]
["3ПБ27-8п",830.5084745762713,665,980,0.072,0.18,"2720*120*220"]
["3ПБ30-8п",880.9322033898305,710,1039.5,0.079,0.2,"2980*120*220"]
["3ПБ34-4п",940.677966101695,750,1110,0.089,0.22,"3370*120*220"]
["3ПБ36-4п",1046.6101694915255,840,1235,0.096,0.24,"3630*120*220"]
["3ПБ39-8п",1478.813559322034,1180,1745,0.103,0.26,"3890*120*220"]
["3ПП14-71п",1233.0508474576272,990,1455,0.119,0.3,"1400*380*220"]
["3ПП16-71п",1546.6101694915255,1239.75,1825,0.13,0.33,"1550*380*220"]
["3ПП18-71п",1966.1016949152543,1580,2320,0.151,0.38,"1810*380*220"]
["3ПП21-71п",2292.3728813559323,1840,2705,0.173,0.43,"2070*380*220"]
["3ПП27-71п",4161.016949152543,3340,4910,0.227,0.57,"2720*380*220"]
["4ПБ30-4п",995.7627118644068,800,1175,0.104,0.26,"2980*120*290"]
["4ПБ44-8п",1838.9830508474577,1480,2170,0.154,0.39,"4410*120*290"]
["4ПБ48-8п",2144.06779661017,1710,2530,0.167,0.42,"4800*120*290"]
["5ПБ18-27п",1211.864406779661,970,1430,0.1,0.25,"1810*250*220"]
["5ПБ18-37п",1521.1864406779662,1220,1795,0.1,0.25,"1810*250*220"]
["5ПБ21-27п",1406.7796610169491,1130,1660,0.114,0.29,"2070*250*220"]
["5ПБ25-37п",1877.1186440677968,1500,2215,0.135,0.34,"2460*250*220"]
["5ПБ25-27п",1770.7627118644068,1425,2089.5,0.135,0.34,"2460*250*220"]
["5ПБ27-37п",2737.2881355932204,2194.5,3230,0.15,0.38,"2720*250*220"]
["5ПБ27-27п",2250,1800,2655,0.15,0.38,"2720*250*220"]
["5ПБ30-27п",2838.5593220338983,2270,3349.5,0.164,0.41,"2980*250*220"]
["5ПБ30-37п",3457.627118644068,2764.5,4080,0.164,0.41,"2980*250*220"]
["5ПБ31-27п",3131.35593220339,2500,3695,0.171,0.43,"3110*250*220"]
["5ПБ34-20п",3237.2881355932204,2600,3820,0.185,0.46,"3370*250*220"]
["5ПБ36-20п",3669.491525423729,2949.75,4330,0.2,0.5,"3630*250*220"]
["8ПБ10-1п",186.4406779661017,145,220,0.011,0.03,"1030*120*90"]
["8ПБ13-1п",220.33898305084747,170,260,0.014,0.04,"1290*120*90"]
["8ПБ16-1п",271.3983050847458,220,320.25,0.017,0.04,"1550*120*90"]
["8ПБ17-2п",288.135593220339,230,340,0.018,0.05,"1680*120*90"]
["8ПБ19-3п",355.93220338983053,285,420,0.021,0.05,"1940*120*90"]
["8ПП 23-7п",1597.2457627118645,1285,1884.75,0.168,0.42,"2330*380*190"]
["8ПП 25-8п",1686.2288135593221,1350,1989.75,0.178,0.45,"2460*380*190"]
["9ПБ13-37п",453.3898305084746,360,535,0.029,0.07,"1290*120*190"]
["9ПБ16-37п",538.3474576271187,435,635.25,0.035,0.09,"1550*120*190"]
["9ПБ18-37п",725.2118644067797,579.5,855.75,0.041,0.1,"1810*120*190"]
["9ПБ18-8п",516.1016949152543,410,609,0.041,0.1,"1810*120*190"]
["9ПБ21-8п",724.5762711864407,470,855,0.047,0.12,"2070*120*190"]
["9ПБ22-3п",567.7966101694916,450,670,0.05,0.13,"2200*120*190"]
["9ПБ25-3п",635.5932203389831,510,750,0.056,0.14,"2460*120*190"]
["9ПБ25-8п",711.8644067796611,570,840,0.056,0.14,"2460*120*190"]
["9ПБ27-8п",800.8474576271187,640,945,0.062,0.16,"2720*120*190"]
["9ПБ30-4п",898.3050847457628,720,1060,0.068,0.17,"2980*120*190"]
["10ПБ21-27п",1500,1200,1770,0.098,0.25,"2070*250*190"]
["10ПБ25-37п",2364.406779661017,1890,2790,0.117,0.29,"2460*250*190"]
["10ПБ27-37п",3775.4237288135596,3030,4455,0.129,0.32,"2460*250*190"]
["ИПР-13",2038.1355932203392,1630,2405,0.176,0.44,"4150*290*250/120"]
["Плиты балконов"]
["ПБК 24.12-5а",4669.491525423729,3930,5510,0.35,0.88,"2390*1240*150/80"]
["ПБК 33.12-5а",5762.71186440678,4830,6800,0.48,1.2,"3290*1240*150/80"]
["ПБК 36.12-5а",6508.474576271186,5450,7680,0.52,1.3,"3590*1240*150/80"]
["ПБК39.12-5а",6779.661016949153,5700,8000,0.54,1.35,"3890*1240*150/80"]
["ПБК42.12-5а",7355.932203389831,6175,8680,0.63,1.58,"4190*1240*150/80"]
["Плиты перекрытий ребристые"]
["1П3-2АIIIвт",11728.813559322034,9860,13840,0.9,2.25,"5550*1485*400"]
["1П3-3АIIIвт",12491.525423728814,10500,14740,0.9,2.25,"5550*1485*400"]
["1П4-5АIIIвт",13317.796610169493,11200,15715,0.83,2.08,"5050*1485*400"]
["2П1-2АIIIвт",13436.440677966102,11300,15855,0.95,2.38,"5950*1485*400"]
["2П1-3АIIIвт",13728.813559322034,11540,16200,0.95,2.38,"5950*1485*400"]
["2П1-4АIIIвт",14025.423728813561,11780,16550,0.95,2.38,"5950*1485*400"]
["2П1-5АIIIвт",17262.71186440678,14500,20370,0.95,2.38,"5950*1485*400"]
["2П1-6АIIIвт",18165.254237288136,15300,21435,0.95,2.38,"5950*1485*400"]
["Плиты покрытий ребристые"]
["2ПГ6-3АтV",6317.796610169492,5320,7455,0.615,1.54,"5970*1490*300"]
["2ПГ6-4АIIIвт",7135.593220338983,6000,8420,0.615,1.54,"5970*1490*300"]
["2ПГ6-5АIIIвт",7737.076271186441,6500,9129.75,0.615,1.54,"5970*1490*300"]
["Плиты покрытий ребристые"]
["ПГ3АтV",11694.915254237289,9830,13800,1.07,2.68,"5970*2980*300"]
["ПГ5АтV",13169.49152542373,11070,15540,1.07,2.68,"5970*2980*300"]
["ПВ10-4АIIIвт",15313.538135593222,12870,18069.975000000002,1.45,3.63,"5970*2980*300"]
["ПР3-51-12-3",4237.28813559322,3560,5000,0.48,1.2,"5080*1190*300"]
["ПР3-51-15-3",4567.796610169492,3850,5390,0.54,1.35,"5080*1490*300"]
["ПР3-63-12-3",5101.6949152542375,4284.5,6020,0.59,1.48,"6280*1190*300"]
["ПР3-63-15-3",5546.610169491526,4664.5,6545,0.67,1.68,"6280*1480*300"]
["Плиты пустотные"]
["ПК24.10-8тва",3144.06779661017,2660,3710,0.29,0.73,"2380*990*220"]
["ПК24.12-8тва",3093.220338983051,2470,3650,0.35,0.88,"2380*1190*220"]
["ПК24.15-8тва",3677.9661016949153,2930,4340,0.46,1.15,"2380*1490*220"]
["ПК27.10-8тва",3504.237288135593,2945,4135,0.33,0.83,"2680*990*220"]
["ПК27.12-8тва",3677.9661016949153,2945,4340,0.39,0.98,"2680*1190*220"]
["ПК27.15-8тва",4470.338983050848,3570,5275,0.52,1.3,"2680*1490*220"]
["ПК28.12-8тва",3677.9661016949153,2900,4340,0.4,1,"2780*1190*220"]
["ПК28.15-8тва",4470.338983050848,3570,5275,0.53,1.33,"2780*1480*220"]
["ПК30.10-8тва",3643.8559322033902,3040,4299.75,0.36,0.9,"2980*990*220"]
["ПК30.12-8тва",3550.4237288135596,2850,4189.5,0.44,1.1,"2980*1190*220"]
["ПК30.15-8тва",4415.254237288136,3530,5210,0.57,1.43,"2980*1490*220"]
["ПК32.10-8тва",3949.1525423728817,3325,4660,0.38,0.95,"3180*990*220"]
["ПК32.12-8тва",4084.322033898305,3250,4819.5,0.46,1.15,"3180*1190*220"]
["ПК32.15-8тва",4868.64406779661,3895,5745,0.61,1.53,"3180*1490*220"]
["ПК33.10-8тва",4389.830508474576,3700,5180,0.39,0.98,"3280*990*220"]
["ПК33.12-8тва",4334.745762711865,3515,5115,0.48,1.2,"3280*1190*220"]
["ПК33.15-8тва",5512.5,4465,6504.75,0.63,1.58,"3280*1490*220"]
["ПК34.10-8тва",4385.593220338983,3719.25,5175,0.41,1.03,"3380*990*220"]
["ПК34.12-8тва",4334.745762711865,3524.5,5115,0.49,1.23,"3380*1190*220"]
["ПК34.15-8тва",5779.449152542373,4600,6819.75,0.65,1.63,"3380*1490*220"]
["ПК36.10-8тва",4262.28813559322,3570,5029.5,0.43,1.08,"3580*990*220"]
["ПК36.12-8тва",4203.389830508475,3360,4960,0.52,1.3,"3580*1190*220"]
["ПК36.15-8тва",5517.171610169493,4400,6510.262500000001,0.69,1.73,"3580*1490*220"]
["ПК38.10-8тва",5254.449152542373,4400,6200.25,0.45,1.13,"3780*990*220"]
["ПК38.12-8тва",5389.830508474576,4360,6360,0.55,1.38,"3780*1190*220"]
["ПК38.15-8тва",6703.389830508475,5400,7910,0.73,1.83,"3780*1490*220"]
["ПК39.12-8тва",5517.171610169493,4465,6510.262500000001,0.57,1.43,"3880*1190*220"]
["ПК39.15-8тва",6838.983050847458,5470,8070,0.74,1.85,"3880*1490*220"]
["ПК40.12-8тва",5779.449152542373,4600,6819.75,0.58,1.45,"3980*1190*220"]
["ПК40.15-8тва",6966.1016949152545,5600,8220,0.76,1.9,"3980*1490*220"]
["ПК42.10-8тва",5385.593220338983,4500,6355,0.5,1.25,"4180*990*220"]
["ПК42.12-8тва",5402.542372881357,4500,6375,0.6,1.5,"4180*1190*220"]
["ПК42.15-8тва",6703.389830508475,5400,7910,0.8,2,"4180*1490*220"]
["ПК43.10-8тва",5966.313559322034,5000,7040.25,0.51,1.28,"4280*990*220"]
["ПК43.12-8тва",6258.474576271186,5000,7385,0.62,1.55,"4280*1190*220"]
["ПК43.15-8тва",7491.525423728814,5985,8840,0.82,2.05,"4280*1490*220"]
["ПК45.10-8тва",5966.313559322034,5000,7040.25,0.53,1.33,"4480*990*220"]
["ПК45.12-8тва",6258.474576271186,5000,7385,0.65,1.63,"4480*1190*220"]
["ПК45.15-8тва",7491.525423728814,5985,8840,0.86,2.15,"4480*1490*220"]
["ПК46.12-8тва",6258.474576271186,5000,7385,0.66,1.65,"4580*1190*220"]
["ПК46.15-8тва",7491.525423728814,5985,8840,0.88,2.2,"4580*1490*220"]
["ПК48.10-8тва",5762.71186440678,4820,6800,0.57,1.43,"4780*990*220"]
["ПК48.12-8тва",5902.542372881357,4750,6965,0.69,1.73,"4780*1190*220"]
["ПК48.15-8тва",7097.457627118644,5700,8375,0.92,2.3,"4780*1490*220"]
["ПК50.12-8АтVа",5779.449152542373,4680,6819.75,0.72,1.8,"4980*1190*220"]
["ПК50.15-8АтVa",8144.06779661017,6555,9610,0.95,2.38,"4980*1490*220"]
["ПК51.10-8АтVа",5885.593220338983,4970,6945,0.6,1.5,"5080*990*220"]
["ПК51.12-8АтVа",6050.847457627119,4870,7140,0.73,1.83,"5080*1190*220"]
["ПК51.15-8АтVа",7750.201271186442,6240,9145.237500000001,0.97,2.43,"5080*1490*220"]
["ПК52.12-8АтVа",7292.383474576272,5840,8605.0125,0.75,1.88,"5180*1190*220"]
["ПК52.15-8АтVа",8809.322033898305,7030,10395,0.99,2.48,"5180*1490*220"]
["ПК53.12-8АтVа",6385.593220338983,5900,7535,0.76,1.9,"5280*1190*220"]
["ПК53.15-8АтVа",7830.5084745762715,7030,9240,1.01,2.53,"5280*1490*220"]
["ПК54.10-8AтVа",6635.593220338983,5600.46375,7830,0.64,1.6,"5380*990*220"]
["ПК54.12-8АтVа",6966.1016949152545,5600.46375,8220,0.78,1.95,"5380*1190*220"]
["ПК54.15-8АтVа",8292.372881355932,6670,9785,1.03,2.58,"5380*1490*220"]
["ПК56.10-8АтVа",6635.593220338983,5600.46375,7830,0.66,1.65,"5580*990*220"]
["ПК56.12-8АтVа",6966.1016949152545,5600.46375,8220,0.81,2.03,"5580*1190*220"]
["ПК56.12-10АтVа",9461.864406779661,7540,11165,0.81,2.03,"5580*1190*220"]
["ПК56.15-8АтVа",8275.42372881356,6670,9765,1.06,2.65,"5580*1490*220"]
["ПК56.15-10АтVа",11436.440677966102,9200,13495,1.06,2.65,"5580*1490*220"]
["ПК57.10-8АтVа",6635.593220338983,5600,7830,0.67,1.68,"5680*990*220"]
["ПК57.10-12,5АтVа",8411.016949152543,6700,9925,0.67,1.68,"5680*990*220"]
["ПК57.12-8АтVа",7063.559322033899,5600,8335,0.82,2.05,"5680*1190*220"]
["ПК57.12-12,5АтVа",9461.864406779661,7609.5,11165,0.82,2.05,"5680*1190*220"]
["ПК57.15-8АтVа",8292.372881355932,6670,9785,1.08,2.7,"5680*1490*220"]
["ПК57.15-12,5АтVа",11516.949152542373,9215,13590,1.08,2.7,"5680*1490*220"]
["ПК58.10-8АтVа",6767.161016949153,5700,7985.25,0.69,1.73,"5780*990*220"]
["ПК58.10-12,5АтVа",8631.35593220339,7220,10185,0.69,1.73,"5780*990*220"]
["ПК.58.12-8AтVa",6966.1016949152545,5605,8220,0.83,2.08,"5780*1190*220"]
["ПК.58.15-8AтVa",8292.372881355932,6670,9785,1.1,2.75,"5780*1490*220"]
["ПК58.12-12,5АтVа",9330.508474576272,7505,11010,0.83,2.08,"5780*1190*220"]
["ПК58.15-12,5АтVа",11597.457627118645,7500,13685,1.1,2.75,"5780*1490*220"]
["ПК59.12-8АтVа",6966.1016949152545,5600,8220,0.85,2.13,"5880*1190*220"]
["ПК59.15-8АтVа",8292.372881355932,6670,9785,1.12,2.8,"5880*1490*220"]
["ПК60.10-8АтVа",6889.830508474577,5800,8130,0.71,1.78,"5980*990*220"]
["ПК60.10-12.5АтVа",8389.830508474577,7030,9900,0.71,1.78,"5980*990*220"]
["ПК60.12-8АтVа",6966.1016949152545,5605,8220,0.86,2.15,"5980*1190*220"]
["ПК60.12-12,5АтVa",7627.118644067797,7140,9000,0.86,2.15,"5980*1190*220"]
["ПК60.15-8АтVа",8292.372881355932,6670,9785,1.14,2.85,"5980*1490*220"]
["ПК60.15-12,5АтVа",11029.671610169493,8870,13015.0125,1.14,2.85,"5980*1490*220"]
["ПК62.12-8АтVа",7296.610169491526,5840,8610,0.89,2.23,"6180*1190*220"]
["ПК62.15-8АтVа",8949.152542372882,7125,10560,1.18,2.95,"6180*1490*220"]
["ПК63.10-8АтVа",7390.042372881357,6240,8720.25,0.74,1.85,"6280*990*220"]
["ПК63.12-8АтVа",7297,5840,8610,0.9,2.25,"6280*1190*220"]
["ПК63.12-12,5АтVа",7881.355932203391,6320,9300,0.9,2.25,"6280*1190*220"]
["ПК63.15-8АтVа",8949.152542372882,7125,10560,1.19,2.98,"6280*1490*220"]
["ПК63.15-12,5АтVа",9860.169491525425,7920,11635,1.19,2.98,"6280*1490*220"]
["П64.10-8АтV-1",7758.474576271187,6500,9155,0.76,1.9,"6380*990*220"]
["П64.12-8АтV-1",7377.118644067797,5899.5,8705,0.91,2.28,"6380*1190*220"]
["П64.15-8АтV-1",9055.084745762711,7270,10685,1.21,3.03,"6380*1490*220"]
["П64.15-12,5АтV-1",11771.186440677966,9880,13890,1.21,3.03,"6380*1490*220"]
["П65.10-8АтV-1",7822.033898305085,6500,9230,0.77,1.93,"6480*990*220"]
["П65.12-8АтV-1",7457.627118644068,5985,8800,0.93,2.33,"6480*1190*220"]
["П65.15-8АтV-1",9161.016949152543,7350,10810,1.23,3.08,"6480*1490*220"]
["П66.10-8АтV-1",7822.033898305085,6500,9230,0.78,1.95,"6580*990*220"]
["П66.12-8АтV-1",7542.372881355933,5985,8900,0.94,2.35,"6580*1190*220"]
["П66.15-8АтV-1",9266.949152542373,7500,10935,1.25,3.13,"6580*1190*220"]
["П67.12-8АтV-1",7635.593220338984,6400,9010,0.96,2.4,"6680*1190*220"]
["П67.15-8АтV-1",9648.305084745763,8075,11385,1.27,3.18,"6680*1490*220"]
["П68.12-8АтV-1",7838.983050847458,6585,9250,0.98,2.45,"6780*1190*220"]
["П68.15-8АтV-1",9766.949152542373,8200,11525,1.29,3.23,"6780*1490*220"]
["П70.12-8АтV-1",7881.355932203391,6640,9300,1,2.5,"6980*1190*220"]
["П70.15-8АтV-1",9953.389830508475,8360,11745,1.33,3.33,"6980*1490*220"]
["1ПК72.10-8АтV",8381.35593220339,7030,9890,0.86,2.15,"7180*990*220"]
["П72.10-12,5АтV-1",10139.618644067798,8550,11964.75,0.86,2.15,"7180*990*220"]
["П72.12-8АтV-1",8008.474576271187,6765,9450,1.03,2.58,"7180*1190*220"]
["П72.12-12,5АтV-1",10139.618644067798,8550,11964.75,1.03,2.58,"7180*1190*220"]
["П72.15-8АтV-1",10139.618644067798,8550,11964.75,1.36,3.4,"7180*1490*220"]
["П73.12-6АтV-1",11830.296610169493,9950,13959.75,1.05,2.63,"7280*1190*220"]
["П73.15-6АтV-1",14771.186440677968,12400,17430,1.38,3.45,"7280*1490*220"]
["П74.12-6АтV-1",12079.449152542373,10165,14253.75,1.06,2.65,"7380*1190*220"]
["1ПК74.12-8АтV",12155.062500000002,10240,14342.973750000001,1.06,2.65,"7380*1190*220"]
["П74.15-6АтV-1",12080.508474576272,12970,14255,1.4,3.5,"7380*1490*220"]
["П75.12-6АтV-1",12156.77966101695,10230,14345,1.07,2.68,"7480*1190*220"]
["1ПК75.12-8АтV",12394.06779661017,10450,14625,1.07,2.68,"7480*1190*220"]
["П75.15-6тV-1",15521.186440677968,13040,18315,1.42,3.55,"7480*1490*220"]
["1ПК75.15-8тV",15661.016949152543,13170,18480,1.42,3.55,"7480*1490*220"]
["П76.12-6АтV-1",12262.71186440678,10355,14470,1.09,2.73,"7580*1190*220"]
["П76.15-6АтV-1",15652.118644067798,13170,18469.5,1.44,3.6,"7580*1490*220"]
["П80.12-6АтV-1",12893.644067796611,10800,15214.5,1.14,2.85,"7980*1190*220"]
["1ПК.80.12-8АтV",13402.542372881357,11300,15815,1.14,2.85,"7980*1490*220"]
["П80.15-6АтV-1",16525.42372881356,13830,19500,1.51,3.78,"7980*1490*220"]
["1ПК80.15-8АтV",16902.54237288136,14250,19945,1.51,3.78,"7980*1490*220"]
["П82.12-6АтV-1",13275.42372881356,11170,15665,1.17,2.93,"8180*1190*220"]
["П82.15-6АтV-1",16779.661016949154,14100,19800,1.55,3.88,"8180*1490*220"]
["П84.12-6АтV-1",13775.423728813561,11520,16255,1.2,3,"8380*1190*220"]
["П84.15-6АтV-1",17156.77966101695,14400,20245,1.59,3.98,"8380*1490*220"]
["П85.12-6АтV-1",13775.423728813561,11590,16255,1.22,3.05,"8480*1190*220"]
["1ПК.85.12-8АтV",14406.77966101695,12100,17000,1.22,3.05,"8480*1190*220"]
["П85.15-6АтV-1",17279.661016949154,14550,20390,1.61,4.03,"8480*1490*220"]
["1ПК.85.15-8АтV",17775.42372881356,14915,20975,1.61,4.03,"8480*1490*220"]
["П90.12.6АтV-1",13402.542372881357,11250,15815,1.28,3.2,"8980*1190*220"]
["1ПК.90.12.8АтV",15025.423728813561,12635,17730,1.28,3.2,"8980*1190*220"]
["П90.15.6АтV-1",16911.228813559323,14250,19955.25,1.7,4.25,"8980*1490*220"]
["1ПК90.15.8АтV",19165.254237288136,16150,22615,1.7,4.25,"8980*1490*220"]
["Плиты теплотрасс"]
["П4-15",432.2033898305085,360,510,0.04,0.1,"570*740*100"]
["П5-8",1622.8813559322034,1380,1915,0.16,0.4,"780*2990*70"]
["П5д-8",491.52542372881356,400,580,0.04,0.1,"780*740*70"]
["П8-8",2508.4745762711864,2140,2960,0.35,0.88,"1160*2990*100"]
["П8д-8",838.9830508474577,710,990,0.09,0.23,"1160*740*100"]
["П11-8/2",2084.7457627118647,1760,2460,0.22,0.55,"1480*1480*100"]
["П11д-8",1275.4237288135594,1070,1505,0.11,0.28,"1480*740*100"]
["П15-8",6110.169491525424,5130,7210,0.65,1.63,"1840*2990*120"]
["П15д-8 (П15д-5)",1877.1186440677968,1520,2215,0.16,0.4,"1840*740*120"]
["П16-15",8220.338983050848,6910,9700,0.99,2.48,"1840*2990*180"]
["ПТ8-11-9",737.2881355932204,610,870,0.079,0.2,"1100*900*80"]
["ПТ8-13-13",1156.7796610169491,970,1365,0.135,0.34,"1300*1300*80"]
["ПТ8-16-14",1529.6610169491526,1280,1805,0.179,0.45,"1600*1400*80"]
["ПТ12,5-8-6",355.93220338983053,300,420,0.038,0.1,"800*600*80"]
["ПТ12,5-11-9",758.4745762711865,579.5,895,0.079,0.2,"1100*900*80"]
["ПТ12,5-13-13",1216.1016949152543,1020,1435,0.135,0.34,"1300*1300*80"]
["ПТ12,5-16-14",1563.5593220338983,1310,1845,0.179,0.45,"1600*1400*80"]
["Плиты забора"]
["ПО-1",5966.313559322034,5000,7040.25,0.55,1.38,"2500*2550"]
["ПО-2",5241.1016949152545,4400,6184.5,0.4,1,"2500*2500"]
["ПО-2а",4766.949152542373,4000,5625,0.473,1.18,"2500*2000"]
["П 5В",5966.313559322034,5000,7040.25,0.5,1.25,"3980*2200"]
["П 6В",7491.525423728814,6300,8840,0.64,1.6,"4000*2500"]
["П 6В а",7610.169491525424,6400,8980,0.64,1.6,"4000*2500"]
["Фундаменты для забора"]
["ФО-2",1428.177966101695,1200,1685.25,0.22,0.55,"900*750*500"]
["ФО 9.9.5.1",1728.813559322034,1450,2040,0.24,0.6,"900*900*500"]
["Прогоны"]
["ПРГ60.2.5-4т",11182.203389830509,9400,13195,0.6,1.5,"5980*200*500"]
["ПРГ32.1.4-4т",2148.305084745763,1800,2535,0.15,0.38,"3180*120*400"]
["ПРГ36.1.4-4т",2610.169491525424,2200,3080,0.17,0.43,"3580*120*400"]
["ПРГ28.1.3-4т",2033.898305084746,1700,2400,0.1,0.25,"2780*120*300"]
["Сваи"]
["С50.30-3",3338.983050847458,2800,3940,0.46,1.15,"5000*300*300"]
["С50.30-6",3580.5084745762715,2970,4225,0.46,1.15,"5000*300*300"]
["С60.30-3",3932.2033898305085,3300,4640,0.55,1.38,"6000*300*300"]
["С60.30-6",4177.754237288136,3500,4929.75,0.55,1.38,"6000*300*300"]
["С60.30-8",4491.525423728814,3770,5300,0.55,1.38,"6000*300*300"]
["С60.30-8 W8",4838.983050847458,4050,5710,0.55,1.38,"6000*300*300"]
["С70.30-6(4;5)",4766.949152542373,3950,5625,0.64,1.6,"7000*300*300"]
["С70.30-8(9)",5622.881355932203,4720,6635,0.64,1.6,"7000*300*300"]
["С70.30-8 W8",5902.542372881357,4980,6965,0.64,1.6,"7000*300*300"]
["С80.30-6",5529.661016949153,4655,6525,0.73,1.83,"8000*300*300"]
["С80.30-8",5987.28813559322,5035,7065,0.73,1.83,"8000*300*300"]
["С80.30-9",6466.1016949152545,5430,7630,0.73,1.83,"8000*300*300"]
["С80.30-10",6486.864406779661,5450,7654.5,0.73,1.83,"8000*300*300"]
["С80.30-11",7974.576271186441,6700,9410,0.73,1.83,"8000*300*300"]
["С80.35-10",8783.898305084746,7390,10365,1,2.5,"8000*350*350"]
["С90.30-6",6110.169491525424,5130,7210,0.82,2.05,"9000*300*300"]
["С90.30-8",6664.830508474577,5600,7864.5,0.82,2.05,"9000*300*300"]
["С90.30-9",7212.076271186441,6060,8510.25,0.82,2.05,"9000*300*300"]
["С90.30-10",7851.6949152542375,6600,9265,0.82,2.05,"9000*300*300"]
["С100.30-6",6822.033898305085,5740,8050,0.91,2.28,"10000*300*300"]
["С100.30-8",7355.932203389831,6175,8680,0.91,2.28,"10000*300*300"]
["С100.30-9",7974.576271186441,6700,9410,0.91,2.28,"10000*300*300"]
["С100.30-11",10105.932203389832,8500,11925,0.91,2.28,"10000*300*300"]
["С110.30-8",8025.826271186442,6745,9470.475,1,2.5,"11000*300*300"]
["С110.30-9",8707.627118644068,7300,10275,1,2.5,"11000*300*300"]
["С100.35-9",10707.627118644068,9000,12635,1.24,3.1,"11000*350*350"]
["С110.30-10",9427.966101694916,7930,11125,1,2.5,"11000*300*300"]
["С120.30-8",8745.762711864407,7350,10320,1.09,2.73,"12000*300*300"]
["С120.35-8 W6",11864.406779661018,9975,14000,1.49,3.73,"12000*350*350"]
["С120.30-8 W6",9165.254237288136,7700,10815,1.09,2.73,"12000*300*300"]
["С120.30-9",9500,7980,11210,1.09,2.73,"12000*300*300"]
["С120.30-10",10279.661016949152,8645,12130,1.09,2.73,"12000*300*300"]
["С120.30-11",11809.322033898306,9930,13935,1.09,2.73,"12000*300*300"]
["Столбы ограждения сигнальные"]
["НС - 1L=1,9",682.2033898305085,570,805,0.05,0.13,"1900*160*160"]
["Ступени"]
["ЛС9",474.5762711864407,400,560,0.0394,0.1,"900*330*148"]
["ЛС11",542.3728813559322,450,640,0.046,0.12,"1050*330*148"]
["ЛС11-1",610.1694915254237,510,720,0.046,0.12,"1050*330*148"]
["ЛСВ 11",673.728813559322,560,795,0.036,0.09,"1050*260*145"]
["ЛСН 11",491.52542372881356,410,580,0.024,0.06,"1160*290*145"]
["ЛС12",597.4576271186442,500,705,0.053,0.13,"1200*330*148"]
["ЛС12-1",648.3050847457628,540,765,0.053,0.13,"1200*330*148"]
["ЛСВ 12",728.8135593220339,610,860,0.041,0.103,"1310*260*145"]
["ЛСН 12 ",542.3728813559322,450,640,0.027,0.068,"1200*290*145"]
["ЛС 14",627.3305084745763,520,740.25,0.06,0.15,"1350*330*148"]
["ЛС 14-1",758.4745762711865,630,895,0.06,0.15,"1350*330*148"]
["ЛСВ 14",822.0338983050848,680,970,0.046,0.115,"1460*260*145"]
["ЛСН 14 ",627.3305084745763,520,740.25,0.031,0.078,"1350*290*145"]
["ЛС 15",656.7796610169491,550,775,0.066,0.17,"1500*330*148"]
["ЛС 15-1",783.8983050847459,660,925,0.066,0.17,"1500*330*148"]
["ЛСВ 15 ",877.1186440677967,730,1035,0.05,0.125,"1610*260*145"]
["ЛСН 15 ",673.728813559322,560,795,0.034,0.085,"1500*290*145"]
["ЛС17",716.3135593220339,600,845.25,0.072,0.18,"1650*330*148"]
["ЛС17-1",834.7457627118645,700,985,0.072,0.18,"1650*330*148"]
["ЛСВ 17",779.6610169491526,650,920,0.055,0.138,"1760*260*145"]
["ЛСН 17 ",610.1694915254237,510,720,0.038,0.095,"1650*290*145"]
["ЛС23",932.2033898305085,780,1100,0.1,0.25,"2250*330*148"]
["ЛС23-1",1101.6949152542375,920,1300,0.1,0.25,"2250*330*148"]
["ЛСВ 23 ",969.9152542372882,810,1144.5,0.074,0.185,"2360*260*145"]
["ЛСН 23 ",779.6610169491526,650,920,0.051,0.13,"2250*290*145"]
["Тротуарная плитка"]
["ТР-2(арм)",144.0677966101695,125,170,0.0125,0.03,"500*500*50"]
["Плиты парапетов"]
["ПП15-60",648.3050847457628,540,765,0.072,0.18,"1490*600*100/60"]
["Утяжитель"]
["УБК-1",null,null,null,2.51,6.28]
["Фундаментные подушки"]
["ФЛ6.12-4",1105.9322033898306,930,1305,0.18,0.45,"1180*600*300"]
["ФЛ6.24-4",2203.389830508475,1860,2600,0.37,0.93,"2380*600*300"]
["ФЛ8.12-3",1432.2033898305085,1200,1690,0.22,0.55,"1180*800*300"]
["ФЛ8.12-4",1529.6610169491526,1280,1805,0.22,0.55,"1180*800*300"]
["ФЛ8.24-3",2707.627118644068,2280,3195,0.46,1.15,"2380*800*300"]
["ФЛ8.24-4",2889.8305084745766,2430,3410,0.46,1.15,"2380*800*300"]
["ФЛ10.8-2",1156.7796610169491,970,1365,0.17,0.43,"780*1000*300"]
["ФЛ10.8-3",1165.2542372881358,980,1375,0.17,0.43,"780*1000*300"]
["ФЛ10.8-4",1190.677966101695,1000,1405,0.17,0.43,"780*1000*300"]
["ФЛ10.12-2",1690.677966101695,1425,1995,0.26,0.65,"1180*1000*300"]
["ФЛ10.12-3",1800.8474576271187,1520,2125,0.26,0.65,"1180*1000*300"]
["ФЛ10.24-2",3173.728813559322,2740,3745,0.55,1.38,"2380*1000*300"]
["ФЛ10.24-3",3376.906779661017,2830,3984.75,0.55,1.38,"2380*1000*300"]
["ФЛ10.24-4",3504.237288135593,2945,4135,0.55,1.38,"2380*1000*300"]
["ФЛ12.8-2",1385.5932203389832,1150,1635,0.2,0.5,"780*1200*300"]
["ФЛ12.8-3",1428.177966101695,1200,1685.25,0.2,0.5,"780*1200*300"]
["ФЛ12.12-2",2033.898305084746,1700,2400,0.31,0.78,"1180*1200*300"]
["ФЛ12.12-3",2148.305084745763,1800,2535,0.31,0.78,"1180*1200*300"]
["ФЛ12.24-2",4449.152542372882,3740,5250,0.65,1.63,"2380*1200*300"]
["ФЛ12.24-3",4669.491525423729,3930,5510,0.65,1.63,"2380*1200*300"]
["ФЛ14.8-2",1550.8474576271187,1300,1830,0.23,0.58,"780*1400*300"]
["ФЛ14.12-2",2313.5593220338983,1950,2730,0.36,0.9,"1180*1200*300"]
["ФЛ14.12-3",2529.661016949153,2130,2985,0.36,0.9,"1180*1200*300"]
["ФЛ14.24-2",4834.745762711865,4060,5705,0.76,1.9,"2380*1400*300"]
["ФЛ14.24-3",5233.050847457627,4400,6175,0.76,1.9,"2380*1400*300"]
["ФЛ16.8-2",1826.271186440678,1520,2155,0.26,0.65,"780*1600*300"]
["ФЛ16.8-3",2084.7457627118647,1760,2460,0.26,0.65,"780*1600*300"]
["ФЛ16.12-2",2741.5254237288136,2300,3235,0.41,1.03,"1180*1600*300"]
["ФЛ16.12-3",3055.084745762712,2565,3605,0.41,1.03,"1180*1600*300"]
["ФЛ16.24-2",5517.171610169493,4635,6510.262500000001,0.86,2.15,"2380*1600*300"]
["ФЛ16.24-3",6300.847457627119,5300,7435,0.86,2.15,"2380*1600*300"]
["ФЛ20.8-2",3059.322033898305,2565,3610,0.5,1.25,"780*2000*500"]
["ФЛ20.8-3",3338.983050847458,2800,3940,0.5,1.25,"780*200*500"]
["ФЛ20.12-2",4758.474576271186,3990,5615,0.78,1.95,"1180*2000*500"]
["ФЛ20.12-3",4923.728813559323,4300,5810,0.78,1.95,"1180*2000*500"]
["ФЛ24.8-2",3635.5932203389834,3035.25,4290,0.58,1.45,"2380*780*500"]
["ФЛ24.8-3",4093.220338983051,3440,4830,0.58,1.45,"2380*780*500"]
["ФЛ24.12-2",5605.932203389831,4700,6615,0.91,2.28,"1180*2400*500"]
["ФЛ24.12-3",6275.42372881356,5250,7405,0.91,2.28,"1180*2400*500"]
["ФЛ28.8-2",4563.559322033899,3840,5385,0.72,1.8,"780*2800*500"]
["ФЛ28.8-3",5186.440677966102,4360,6120,0.72,1.8,"780*2800*500"]
["ФЛ28.12-2",7076.271186440678,5950,8350,1.13,2.83,"1180*2800*500"]
["ФЛ28.12-3",7919.491525423729,6650,9345,1.13,2.83,"1180*2800*500"]
["ФЛ32.8-2",5652.542372881357,4750,6670,0.82,2.05,"780*3200*500"]
["ФЛ32.8-3",6664.830508474577,5600,7864.5,0.83,2.08,"780*3200*500"]
["ФЛ32.12-2",8771.186440677966,7350,10350,1.29,3.23,"1180*3200*500"]
["ФЛ32.12-3",10105.932203389832,8500,11925,1.29,3.23,"1180*3200*500"]
["Утяжелитель"]
["УБО",null,null,null,0.94,2.35]
["УБК-1",null,null,null,2.51,6.28]
["Бордюр, поребрик , брусчатка"]
["БР100.30.15",203.38983050847457,170,240,0.043,0.11,"1000*300*150"]
["СКЦ-1",55.08474576271187,null,65,0.011,0.023,"390*190*188"]
["СКЦ-2",42.37288135593221,null,50,0.007,0.015,"390*190*188"]
["ЭДД(красная)       1м2",419.49152542372883,null,495,0.0014,0.003,"200*100*70"]
["ЭДД(серая)           1м2",338.98305084745766,285,400,0.0014,0.003,"200*100*70"]
[]
["Сетка из пров.&5",34915.254237288136,34000,41200,1,1]
["Блоки фундаментов"]
["ФБС24.3.6т",1339.1949152542375,1235,1580.25,0.406,0.97,"2380*300*580"]
["ФБС24.4.6т",1618.6440677966102,1500,1910,0.543,1.3,"2380*400*580"]
["ФБС24.5.6т",2016.949152542373,1860,2380,0.679,1.63,"2380*500*580"]
["ФБС24.6.6т",2402.542372881356,2240,2835,0.815,1.96,"2380*600*580"]
["ФБС 12.3.6т",754.2372881355933,630,890,0.203,0.49,"1180*300*580"]
["ФБС 12.4.6т",970.3389830508476,800,1145,0.265,0.64,"1180*400*580"]
["ФБС 12.5.6т",1186.4406779661017,1000,1400,0.331,0.79,"1180*500*580"]
["ФБС 12.6.6т",1427.9661016949153,1200,1685,0.398,0.96,"1180*600*580"]
["ФБС 12.4.3т",512.7118644067797,430,605,0.127,0.3,"1180*400*280"]
["ФБС 12.5.3т",627.1186440677966,520,740,0.159,0.38,"1180*500*280"]
["ФБС 12.6.3т",588.9830508474577,579.5,695,0.191,0.46,"1180*600*280"]
["ФБС 9.3.6т",567.7966101694916,450,670,0.146,0.35,"880*300*580"]
["ФБС 9.4.6т",754.2372881355933,600,890,0.195,0.47,"880*400*580"]
["ФБС 9.5.6т",932.2033898305085,730,1100,0.244,0.59,"880*500*580"]
["ФБС9.6.6т",1135.5932203389832,900,1340,0.293,0.7,"880*600*580"]